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	Name
	Description
	Sales Price
	Qty
	Total
	Shipping Origin
	Lead time

	1
	
	G.E or Waygate Technologies
	USD 0.00
	2
	USD 0.00
	
	

	2
	PRBT-RFT-DDST-180HF-N20
	RFT rigid dual driver probe, ABS/DIF, Ø 18 mm, HF, 20 m nylon cable
	USD 4,755.00
	2
	USD 9,510.00
	Eddyfi Quebec
Plant
	70 days

	3
	PRBT-MFL-ADT-194-N20
	MFL rigid probe, ABS, DIF and TRAIL channels, with high resistance replaceable wear rings, diameter 19.4 mm, 20 m premium nylon cable for 19-pin connector. No ABS drift adaptor box required.
	USD 5,180.50
	2
	USD 10,361.00
	Eddyfi Quebec
Plant
	70 days

	4
	PRBT-RFT-DDST-200HF-N20
	RFT rigid dual driver probe, ABS/DIF, Ø 20 mm, HF, 20 m nylon cable
	USD 4,755.00
	2
	USD 9,510.00
	Eddyfi Quebec
Plant
	70 days

	5
	PRBT-RFT-DDST-190HF-N30
	RFT rigid dual driver probe, ABS/DIF, Ø 19 mm, HF, 30 m nylon cable
	USD 5,025.00
	2
	USD 10,050.00
	Eddyfi Quebec
Plant
	70 days

	6
	PRBT-RFT-DDST-240MF-N20
	RFT rigid dual driver probe, ABS/DIF, Ø 24 mm, MF, 20 m nylon cable
	USD 4,755.00
	2
	USD 9,510.00
	Eddyfi Quebec
Plant
	70 days

	7
	PRBT-MFL-ADT-256-N20
	MFL rigid probe, ABS, DIF and TRAIL channels, with high resistance replaceable wear rings, diameter 25.6 mm, 20 m premium nylon cable for 19-pin connector. No ABS drift adaptor box required.
	USD 6,125.00
	2
	USD 12,250.00
	Eddyfi Quebec
Plant
	70 days

	8
	PRBT-NFT-BBAD-130MF-N20
	NFT rigid probe, ABS/DIF, diameter 13.0 mm, MF frequency range, 20 m nylon cable.
	USD 4,615.00
	2
	USD 9,230.00
	Eddyfi Quebec
Plant
	70 days

	9
	PRBT-MFL-ADT-138-N20
	MFL rigid probe, ABS, DIF and TRAIL channels, with high resistance replaceable wear rings, diameter 13.8 mm, 20 m premium nylon cable for 19-pin connector. No ABS drift adaptor box required, limited OD detection.
	USD 5,985.00
	2
	USD 11,970.00
	Eddyfi Quebec
Plant
	70 days

	10
	PRBT-NFT-BBAD-140MF-N20
	NFT rigid probe, ABS/DIF, diameter 14.0 mm, MF frequency range, 20 m nylon cable.
	USD 4,615.00
	2
	USD 9,230.00
	Eddyfi Quebec
Plant
	70 days

	11
	PRBT-MFL-ADT-148-N20
	MFL rigid probe, ABS, DIF and TRAIL channels, with high resistance replaceable wear rings, diameter 14.8 mm, 20 m premium nylon cable for 19-pin connector. No ABS drift adaptor box required, limited OD detection.
	USD 5,985.00
	2
	USD 11,970.00
	Eddyfi Quebec
Plant
	70 days

	12
	PRBT-MFL-ADT-200-N20
	MFL rigid probe, ABS, DIF and TRAIL channels, with high resistance replaceable wear rings, diameter 20.0 mm, 20 m premium nylon cable for 19-pin connector. No ABS drift adaptor box required.
	USD 5,985.00
	2
	USD 11,970.00
	Eddyfi Quebec
Plant
	70 days

	13
	DEFHI-ERBCA-200LF-N05
	DefHi® ECA probe with bobbin, circumferential array, and axial array. Rigid design, 20 mm 
diameter, LF 20-200 kHz frequency range, 5 m nylon cable. Comes with the Ectane® 160-pin connector and requires the Ectane® 128 option.
	USD 11,589.50
	2
	USD 23,179.00
	Eddyfi Quebec
Plant
	70 days



